
diff -r 6787754b251b -r b6572d0336c3 doc/doxygen/latex/structcan__baudparams__t.tex
--- /dev/null	Thu Jan 01 00:00:00 1970 +0000
+++ b/doc/doxygen/latex/structcan__baudparams__t.tex	Mon Jun 04 17:59:50 2007 +0200
@@ -0,0 +1,70 @@
+\hypertarget{structcan__baudparams__t}{
+\section{can\_\-baudparams\_\-t Struct Reference}
+\label{structcan__baudparams__t}\index{can_baudparams_t@{can\_\-baudparams\_\-t}}
+}
+{\tt \#include $<$lincan.h$>$}
+
+\subsection*{Data Fields}
+\begin{CompactItemize}
+\item 
+long \hyperlink{structcan__baudparams__t_6186d236aabd8604eb9d39f518b014fa}{flags}
+\item 
+long \hyperlink{structcan__baudparams__t_b9e5b5418206d02cc1ff852b6bc61d5e}{baudrate}
+\item 
+long \hyperlink{structcan__baudparams__t_a81e104a371b1efc2cc08031afac924c}{sjw}
+\item 
+long \hyperlink{structcan__baudparams__t_b5d2e0ccd2e1f474d9e9d08d3d7fa9ed}{sample\_\-pt}
+\end{CompactItemize}
+
+
+\subsection{Detailed Description}
+struct \hyperlink{structcan__baudparams__t}{can\_\-baudparams\_\-t} - datatype for calling CONF\_\-BAUDPARAMS IOCTL : reserved for additional flags for chip configuration, should be written -1 or 0 : baud rate in Hz : synchronization jump width (0-3) prescaled clock cycles : sample point in \% (0-100) sets (TSEG1+1)/(TSEG1+TSEG2+2) ratio
+
+The structure is used to configure new set of parameters into CAN controller chip. If default value of some field should be preserved, fill field by value -1. 
+
+
+
+Definition at line 49 of file lincan.h.
+
+\subsection{Field Documentation}
+\hypertarget{structcan__baudparams__t_6186d236aabd8604eb9d39f518b014fa}{
+\index{can_baudparams_t@{can\_\-baudparams\_\-t}!flags@{flags}}
+\index{flags@{flags}!can_baudparams_t@{can\_\-baudparams\_\-t}}
+\subsubsection[flags]{\setlength{\rightskip}{0pt plus 5cm}long \hyperlink{structcan__baudparams__t_6186d236aabd8604eb9d39f518b014fa}{can\_\-baudparams\_\-t::flags}}}
+\label{structcan__baudparams__t_6186d236aabd8604eb9d39f518b014fa}
+
+
+
+
+Definition at line 50 of file lincan.h.\hypertarget{structcan__baudparams__t_b9e5b5418206d02cc1ff852b6bc61d5e}{
+\index{can_baudparams_t@{can\_\-baudparams\_\-t}!baudrate@{baudrate}}
+\index{baudrate@{baudrate}!can_baudparams_t@{can\_\-baudparams\_\-t}}
+\subsubsection[baudrate]{\setlength{\rightskip}{0pt plus 5cm}long \hyperlink{structcan__baudparams__t_b9e5b5418206d02cc1ff852b6bc61d5e}{can\_\-baudparams\_\-t::baudrate}}}
+\label{structcan__baudparams__t_b9e5b5418206d02cc1ff852b6bc61d5e}
+
+
+
+
+Definition at line 51 of file lincan.h.\hypertarget{structcan__baudparams__t_a81e104a371b1efc2cc08031afac924c}{
+\index{can_baudparams_t@{can\_\-baudparams\_\-t}!sjw@{sjw}}
+\index{sjw@{sjw}!can_baudparams_t@{can\_\-baudparams\_\-t}}
+\subsubsection[sjw]{\setlength{\rightskip}{0pt plus 5cm}long \hyperlink{structcan__baudparams__t_a81e104a371b1efc2cc08031afac924c}{can\_\-baudparams\_\-t::sjw}}}
+\label{structcan__baudparams__t_a81e104a371b1efc2cc08031afac924c}
+
+
+
+
+Definition at line 52 of file lincan.h.\hypertarget{structcan__baudparams__t_b5d2e0ccd2e1f474d9e9d08d3d7fa9ed}{
+\index{can_baudparams_t@{can\_\-baudparams\_\-t}!sample_pt@{sample\_\-pt}}
+\index{sample_pt@{sample\_\-pt}!can_baudparams_t@{can\_\-baudparams\_\-t}}
+\subsubsection[sample\_\-pt]{\setlength{\rightskip}{0pt plus 5cm}long \hyperlink{structcan__baudparams__t_b5d2e0ccd2e1f474d9e9d08d3d7fa9ed}{can\_\-baudparams\_\-t::sample\_\-pt}}}
+\label{structcan__baudparams__t_b5d2e0ccd2e1f474d9e9d08d3d7fa9ed}
+
+
+
+
+Definition at line 53 of file lincan.h.
+
+The documentation for this struct was generated from the following file:\begin{CompactItemize}
+\item 
+/home/epimerde/documents/tc11/Can\-Festival-3/drivers/can\_\-lincan/\hyperlink{lincan_8h}{lincan.h}\end{CompactItemize}




