\hypertarget{structcan__baudparams__t}{
\section{can\_\-baudparams\_\-t Struct Reference}
\label{structcan__baudparams__t}\index{can_baudparams_t@{can\_\-baudparams\_\-t}}
}
{\tt \#include $<$lincan.h$>$}

\subsection*{Data Fields}
\begin{CompactItemize}
\item 
long \hyperlink{structcan__baudparams__t_6186d236aabd8604eb9d39f518b014fa}{flags}
\item 
long \hyperlink{structcan__baudparams__t_b9e5b5418206d02cc1ff852b6bc61d5e}{baudrate}
\item 
long \hyperlink{structcan__baudparams__t_a81e104a371b1efc2cc08031afac924c}{sjw}
\item 
long \hyperlink{structcan__baudparams__t_b5d2e0ccd2e1f474d9e9d08d3d7fa9ed}{sample\_\-pt}
\end{CompactItemize}


\subsection{Detailed Description}
struct \hyperlink{structcan__baudparams__t}{can\_\-baudparams\_\-t} - datatype for calling CONF\_\-BAUDPARAMS IOCTL : reserved for additional flags for chip configuration, should be written -1 or 0 : baud rate in Hz : synchronization jump width (0-3) prescaled clock cycles : sample point in \% (0-100) sets (TSEG1+1)/(TSEG1+TSEG2+2) ratio

The structure is used to configure new set of parameters into CAN controller chip. If default value of some field should be preserved, fill field by value -1. 



Definition at line 49 of file lincan.h.

\subsection{Field Documentation}
\hypertarget{structcan__baudparams__t_6186d236aabd8604eb9d39f518b014fa}{
\index{can_baudparams_t@{can\_\-baudparams\_\-t}!flags@{flags}}
\index{flags@{flags}!can_baudparams_t@{can\_\-baudparams\_\-t}}
\subsubsection[flags]{\setlength{\rightskip}{0pt plus 5cm}long \hyperlink{structcan__baudparams__t_6186d236aabd8604eb9d39f518b014fa}{can\_\-baudparams\_\-t::flags}}}
\label{structcan__baudparams__t_6186d236aabd8604eb9d39f518b014fa}




Definition at line 50 of file lincan.h.\hypertarget{structcan__baudparams__t_b9e5b5418206d02cc1ff852b6bc61d5e}{
\index{can_baudparams_t@{can\_\-baudparams\_\-t}!baudrate@{baudrate}}
\index{baudrate@{baudrate}!can_baudparams_t@{can\_\-baudparams\_\-t}}
\subsubsection[baudrate]{\setlength{\rightskip}{0pt plus 5cm}long \hyperlink{structcan__baudparams__t_b9e5b5418206d02cc1ff852b6bc61d5e}{can\_\-baudparams\_\-t::baudrate}}}
\label{structcan__baudparams__t_b9e5b5418206d02cc1ff852b6bc61d5e}




Definition at line 51 of file lincan.h.\hypertarget{structcan__baudparams__t_a81e104a371b1efc2cc08031afac924c}{
\index{can_baudparams_t@{can\_\-baudparams\_\-t}!sjw@{sjw}}
\index{sjw@{sjw}!can_baudparams_t@{can\_\-baudparams\_\-t}}
\subsubsection[sjw]{\setlength{\rightskip}{0pt plus 5cm}long \hyperlink{structcan__baudparams__t_a81e104a371b1efc2cc08031afac924c}{can\_\-baudparams\_\-t::sjw}}}
\label{structcan__baudparams__t_a81e104a371b1efc2cc08031afac924c}




Definition at line 52 of file lincan.h.\hypertarget{structcan__baudparams__t_b5d2e0ccd2e1f474d9e9d08d3d7fa9ed}{
\index{can_baudparams_t@{can\_\-baudparams\_\-t}!sample_pt@{sample\_\-pt}}
\index{sample_pt@{sample\_\-pt}!can_baudparams_t@{can\_\-baudparams\_\-t}}
\subsubsection[sample\_\-pt]{\setlength{\rightskip}{0pt plus 5cm}long \hyperlink{structcan__baudparams__t_b5d2e0ccd2e1f474d9e9d08d3d7fa9ed}{can\_\-baudparams\_\-t::sample\_\-pt}}}
\label{structcan__baudparams__t_b5d2e0ccd2e1f474d9e9d08d3d7fa9ed}




Definition at line 53 of file lincan.h.

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
/home/epimerde/documents/tc11/Can\-Festival-3/drivers/can\_\-lincan/\hyperlink{lincan_8h}{lincan.h}\end{CompactItemize}
